/dts-v1/;

#include <tactility/bindings/root.h>
#include <tactility/bindings/esp32_gpio.h>
#include <tactility/bindings/esp32_i2c.h>

/ {
	compatible = "root";
	model = "Elecrow CrowPanel Basic 3.5";

	gpio0 {
		compatible = "espressif,esp32-gpio";
		gpio-count = <40>;
	};

	i2c0 {
		compatible = "espressif,esp32-i2c";
		port = <I2C_NUM_0>;
		clock-frequency = <400000>;
		pin-sda = <22>;
		pin-scl = <21>;
		pin-sda-pullup;
		pin-scl-pullup;
	};
};
